

Software Safety Requirements and Architecture

Lane Assistance

**Document Version: [Version]**

**Template Version 1.0, Released on 2017-06-21**



# Document history

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Editor | Description |
| 06/13/2018 | 1.0 | Swapnil More | First Draft |
| 06/15/2018 | 1.1 | Swapnil More | Updates to First Draft |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Table of Contents

[Document history](#_1t3h5sf)

[Table of Contents](#_pyp8fd3vpmy3)

[Purpose](#_c1lz2bx22jid)

[Inputs to the Software Requirements and Architecture Document](#_hjpgfzcjxim1)

[Technical safety requirements](#_lc6owg9q3amb)

[Refined Architecture Diagram from the Technical Safety Concept](#_db3hhee81tpq)

[Software Requirements](#_pul4igmpfvr0)

[Refined Architecture Diagram](#_b7fyegncumoz)

# Purpose

This document identifies the new requirements for the software components at a component level to identify potential problems on software design and architecture that could lead to a violation of safety goals. These requirements are more detail oriented than the technical safety concept requirements.

# Inputs to the Software Requirements and Architecture Document

## Technical safety requirements

Technical Safety Requirements related to Functional Safety Requirement 01-01 are:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Architecture Allocation** | **Safe State** |
| Technical  Safety  Requirement  01-01-01 | The LDW safety component shall ensure that the amplitude of the ‘LDW\_Torque\_Request’ sent to the ‘Final electronic power steering Torque’ component is below ‘Max\_Torque\_Amplitude.’ | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |
| Technical  Safety  Requirement  01-01-02 | When the LDW is  deactivated, the ‘LDW  Safety’ software module  shall send a signal to the  Car Display ECU to turn  on a warning signal. | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |
| Technical  Safety  Requirement  01-01-03 | When a failure is  detected by the Lane  Departure Warning  functionality, it shall  deactivate the Lane  Departure Warning  feature and set  ‘LDW\_Torque\_Request’  to zero. | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |
| Technical  Safety  Requirement  01-01-04 | The validity and integrity  of the data transmission  for  ‘LDW\_Torque\_Request’ signal shall be ensured. | C | 50 ms | Data Transmission Integrity Check | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |
| Technical  Safety  Requirement  01-01-05 | Memory test shall be  conducted at startup of  the EPS ECU to check  for any memory problems | A | Ignition cycle | Memory Test | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

## Refined Architecture Diagram from the Technical Safety Concept

****

# Software Requirements

**Lane Departure Warning (LDW) Amplitude Malfunction Software Requirements:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-01 | The LDW safety component shall ensure that the amplitude of the ‘LDW\_Torque\_Request’ sent to the ‘Final electronic power steering Torque’ component is below ‘Max\_Torque\_Amplitude.’ | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ID | Software Safety Requirement | ASIL | Allocation Software Elements | Safe State |
| Software  Safety  Requirement  01-01-01-01 | The input signal ‘Primary\_LDW\_Torq\_Req’ shall be read and pre-processed to determine the torque request coming from the ‘Basic/Main LAFunctionality’ SW Component. Signal ‘processed\_LDW\_Torq\_Req’ shall be generated at the end of the processing. | C | LDW\_SAGETY\_INPUT\_PROCESSING | N/A |
| Software Safety Requirement 01-01-01-02 | In case the ‘processed\_LDW\_Torq\_Req’ signal has a value greater than ‘Max\_Torque\_Amplitude\_LDW’ (maximum allowed safe torque), the torque signal ‘limited\_LDW\_Torq\_Req’ shall be set to zero, else ‘limited\_LDW\_Torq\_Req’ shall take the value of ‘processed\_LDW\_Torq\_Req’ | C | TORQUE\_LIMITER | ‘limited\_LDW\_Torq\_Req’ = 0 (Nm=Newton-meter) |
| Software Safety Requirement 01-01-01-03 | The ‘limited\_LDW\_Torq\_Req’ shall be transformed into a signal ‘LDW\_Torq\_Req’ which is suitable to be transmitted outside the LDW Safety component (‘LDW Safety’) to the ‘Final EPS Torque’ component. | C | LDW\_SAFETY\_OUTPUT\_GENERATOR | LDW\_Torq\_Req = 0 (Nm) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-02 | When the LDW is  deactivated, the ‘LDW  Safety’ software module  shall send a signal to the  Car Display ECU to turn  on a warning signal. | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-01-02-01 | Any data to be transmitted outside of the LDW Safety component (“LDW Safety”) including "LDW\_Torque\_Req" and “activation\_status” (see SofSafReq03-02) shall be protected by an End2End(E2E) protection mechanism | C | E2ECalc | LDW\_Torq\_Req= 0 (Nm) |
| Software Safety Requirement 01-01-02-02 | The E2E protection protocol shall contain and attach the control data: alive counter (SQC) and CRC to the data to be transmitted. | C | E2ECalc | LDW\_Torq\_Req = 0 (Nm) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-03 | When a failure is  detected by the Lane  Departure Warning  functionality, it shall  deactivate the Lane  Departure Warning  feature and set  ‘LDW\_Torque\_Request’  to zero. | C | 50 ms | LDW Safety | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-01-03-01 | Each of the SW elements shall output a signal to indicate any error which is detected by the element. Error signal = error\_status\_input(LDW\_SAFETY\_INPUT\_PROCESSING), error\_status\_torque\_limiter(TORQUE\_LIMITER), error\_status\_output\_gen(LDW\_SAFETY\_OUTPUT\_GENERATOR) | C | All | N/A |
| Software Safety Requirement 01-01-03-02 | A software element shall evaluate the error status of all the other software elements and in case any 1 of them indicates an error, it shall deactivate the LDW feature (“activation\_status”=0) | C | LDW\_SAFETY\_ACTIVATION | Activation\_status = 0 (LDW function deactivated) |
| Software Safety Requirement 01-01-03-03 | A software element shall evaluate the error status of all the other software elements and in case any 1 of them indicates an error, it shall deactivate the LDW feature (“activation\_status”=0) | C | LDW\_SAFETY\_ACTIVATION | N/A |
| Software Safety Requirement 01-01-03-04 | In case an error is detected by any of the software elements, it shall set the value of its corresponding torque to 0 so that “LDW\_Torq\_Req” is set to 0 | C | All | LDW\_Torq\_Req = 0 |
| Software Safety Requirement 01-01-03-05 | Once the LDW functionality has been deactivated, it shall stay deactivated till the time the ignition is switched from off to on again. | C | LDW\_SAFETY\_ACTIVATION | Activation\_status = 0 (LDW function deactivated) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-04 | The validity and integrity  of the data transmission  for  ‘LDW\_Torque\_Request’ signal shall be ensured. | C | 50 ms | Data Transmission Integrity Check | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-01-04-01 | When the LDW function is deactivated (activation\_status set to 0), the activation\_status shall be sent to the car displayECU. | C | LDW\_SAFETY\_ACTIVATION, CarDisplay ECU | N/A |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ID** | **Technical Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Allocation to Architecture** | **Safe State** |
| Technical  Safety  Requirement  01-01-05 | Memory test shall be  conducted at startup of  the EPS ECU to check  for any memory problems | A | Ignition cycle | Memory Test | Lane  Departure  Warning  Torque Request Amplitude shall be set to  zero. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Software Safety Requirement** | **ASIL** | **Allocation Software Elements** | **Safe State** |
| Software Safety Requirement 01-01-05-01 | A CRC verification check over the software code in the Flash memory shall be done every time the ignition is switched from off to on to check for any content corruption. | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-01-05-02 | Standard RAM test to check the data bus, address bus and device integrity shall be done every time the ignition is switched from off to on (e. G. walking 1s test, RAM pattern test, Refer to RAM and processor vendor recommendations) | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-01-05-03 | The test result of the RAM or Flash memory shall be indicated to the LDW\_Safety component via the ‘test\_status’ signal. | A | MEMORYTEST | Activation\_status = 0 |
| Software Safety Requirement 01-01-05-04 | In case any fault is indicated via the ‘test\_status’ signal the INPUT\_LDW\_PROCESSING shall set an error on the error\_status\_input(=1) so that the Lane Departure Warning functionality is deactivated and the LDW\_Torque\_Req is set to zero. | A | LDW\_SFETY\_INPUT\_PROCESSING | Activation\_status = 0 |

# Refined Architecture Diagram

****